**DS-1227ZJ-P1**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Inceiling MountFeature* Metal plate & plastic with surface spray treatment
* Easy installation method

Dimension**Available Model**DS-1227ZJ-P1Parameter

|  |  |
| --- | --- |
| ModelParameters | DS-1227ZJ-P1 |
| Inceiling Mount |
| Appearance | Hikvision White |
| Material | Metal Plate & Plastic |
| Dimension | Ø 253.4 mm × 38.4 mm (Ø 9.97" × 1.51") |
| Weight | 460 g (1.01 lb.) |

Note* The mount should be installed in the flat ceiling.
* he ceiling must be capable of supporting at least 3 times as much as the total weight of the camera, and the mount.
* The mount’s maximum load capacity is 1 kg (2.2 lb.).
 |

0100001080615